[bookmark: _GoBack][image: A group of black objects

AI-generated content may be incorrect.]

[image: A black rectangular device with a light on it

AI-generated content may be incorrect.]
[image: A diagram of a remote control

AI-generated content may be incorrect.]
[image: A diagram of a computer security system

AI-generated content may be incorrect.][image: A person driving a car

AI-generated content may be incorrect.]
image5.png
150 FeetWorking Range

* 850LM/8B0LM/STAR1000 receivers

Work with - Gate operators
« LiftMaster commercial door operators





image1.png




image2.png




image3.png
Dual 12-Cade
DIP Switch

Securitys 200
Technology

Narowband
Transmission

Technology

Visor Clip .

LED Transmission
LightBatery ndicator

Program Button





image4.png
o
Steps 01

* Setthe D Swiches
opente cverad st 0 0P
switches o oor desired posion
(oNer o7

Steps 02
okt sy e
| WOFPRESSES DEVICESECURITYTYPE
v e
A e
: oo

e ———

Sty 2 Exysed O8]

« ressthe Progrom Butn, thn
press e remotecontrolbuton
accoring toyour e’ oy
‘ype. nenhad e Program
Butonunt e LD on the
renot s oft

Steps 03

= Program the Remate 10 a Device
Prssond eleas th Loam buttenon
your dvice, then itin 30 sconds,
prss and hold the esied butonon
the emot convol 0 s the newly
programned remot btion

- The 811K remote cannotclone remote with e #1 dp itch o o any itches I the midle or 0 postion.
(VYRR ! st emsieisecud it 41 suchon you s progrm the Sl s
10 ensure compatbiltywith oth old and now emotes.
+ Remotes wihout th #1 switch n o any Swiches i the middle osio will ot encunter s isue.

How to replace the

battery

Use a small screwdriver
orvisor clips toopenthe
remote control from the
recess inorder toreplace
the battery.





